Rib Mesh Transferred Electronic Jacquard Circular Knitting Machine

Model HFRT Diameter 30-38" Gauge 12-18G Feeder 48-60F Motor 5.5KW

* **Machine description**

Rib Mesh Transferred Electronic Jacquard Circular Knitting Machine produces appealing Eyelet-effects permit the use of those knit fabrics in gauges up to G18. Rib mesh fabrics is good for underwear and fashionable sportswear.

* **Machine Features**

1. Professional designed CAM system with high speed make sure needles with long life.
2. The rib mesh transferred knitting machine base plate is made of steel ball runway structure with oil immersion, which guarantee the machine with stable running, low noise and high abrasion resistant.
3. Transfer rib jacquard machine equipped with exclusive jacquard electronic feeders to enhance fabric quality.
4. Components and parts for driving system of rib mesh transfer jacquard machine is made by superior material through high efficient heat treatment. Gear and other main components are made in Taiwan and bearing are imported from Japan. All of these make the machine with high precision drive system, low running noise and stable operation.
5. Material of cylinder for rib mesh transferred knitting machine is stainless steel which is imported from Japan, which make sure the cylinder have high quality and good performance.

* **Product application**

Underwear, sportswear etc.

* **Fabric Samples**