Body Size Single Jersey Circular Knitting Machine

Model HFBS Diameter 12-24" Gauge 16-32G Feeder 3F/Inch Motor 2.2-3.7KW

* **Body size single jersey circular knitting machine**specialize in knitting seamless body size fabric for making t-shirt, underwear etc. The seamless fabric makes people feel more comfortable and relax.
* Body Size Single Jersey Circular Knitting Machine equip with 4 track CAM on the cylinder which are 2 track knit CAM, 1 track tuck CAM and 1 track miss CAM.  If you need 2 track CAM only, then groz-beckert needle can be changed to shorter needle.
* The cylinder needle cam system for each feed-contained in a single replaceable section and having an exterior adjustment for the stitch cam slide.
* Material of cylinder for Body Size Single Jersey Circular Knitting Machine is stainless steel which is imported from Japan, which make sure the cylinder have high quality and good performance.
* Components for drive system is made by superior material through high efficient heat treatment. Gear and other main components are made in Taiwan and bearing are imported from Japan. All of these guarantee the machine with high precision drive system, low running noise and stable operation.
* The bed plate for seamless Body Size Single Jersey Circular Knitting Machine is made of steel ball runway structure with oil immersion, which make sure the machine with stable running, low noise and high abrasion resistant.